# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Dark Matter

# FDOS v1.0 FINAL - B57 udiag

- 1
- 2
…
- 97
- 98
- 99
- 100
- 101
…
- 192
- 193

Broadcom NetXtreme Ethernet Adapter • Diagnostic User’s Guide
page 99
Broadcom Confidential and Proprietary
10.42 secfg2
Command: secfg2
Description: Configure NVRAM Group 2
Syntax: secfg2
Options:
-e Engineering Change
-s Serial Number
-m Manufacturing ID
-a Asset Tag
-r Part Rev
-v Voltage
-f Force PCI Mode 1:Enable 2:Disable
10.43 secfg3
Command: secfg3
Description: Configure NVRAM Group 3
Syntax: secfg3
Options:
-l Led Mode 0:Mac 1:Phy1 2:Phy2 3:S Traffic 4:Shasta Mac 5:Wireless Combo
-r Max PCI Retry 0-7, 8:Auto
-a ASF 1:Enable 2:Disable
-d Dual Mac 0:Norm 1:MacB 2:MacA 3:XBAR 4:Swap 7:SwapXBAE
-m MBA Boot Protocol 0:PXE 1:RPL 2:BOOTP 3:ISCSI 4:NONE
-b MBA Bootstrap Type 0:Auto 1:BBS 2:Int18 3:Int19
-t MBA Delay Time 0-15
-e Exp ROM 0:64K 1:128K 2:256K 3:512K 4:1M 5:2M 6:4M 7:8M 8:16M

- 1
- 2
…
- 97
- 98
- 99
- 100
- 101
…
- 192
- 193