# Vault 7: Projects

This publication series is about specific projects related to the Vault 7 main publication.

### Cherry Blossom

# CherryBomb -- CherryBlossom FAT Procedures (CDRL-14a)

8 August, 2012

- 1
- 2
…
- 13
- 14
- 15
- 16
- 17
…
- 79
- 80

UNCLASSIFIED
Cherry Bomb Program Cherry Blossom FAT Procedures
Step Action
1 Setup the Flytrap, Hub, and Squid Laptop (see “Test Diagram”
above):
1. Connect Ethernet cable from Flytrap WAN port to hub
2. Connect Ethernet cable from Squid Laptop to Hub
3. Connect Ethernet cable from Hub (uplink port) to Wired
Internet Access Port
2 Log on to the Squid Laptop (user=squid_user password=squid123!).
Ensure the default connection type for the wired interface is DHCP.
3 Connect the Squid Laptop to the internet (there may be some type of
registration/internet access procedure required at the site). Verify
internet connectivity by going to a web site (e.g., www.google.com).
4 Fetch the Squid Laptop’s IP address (open a terminal window and
issue “ifconfig eth0”) and DNS address(es) (open a terminal, issue
“cat /etc/resolv.conf”, and look for IP address with “nameserver” tag).
5 Start squid on the Squid Laptop. Open a terminal window (as
“squid_user”) and run:
./squid_start.sh
6 Configure the Flytrap’s Internet (WAN) Connection:
a. Boot the Target Laptop in Windows XP and logon
(user=Administrator password=target123!).
b. Connect the Target laptop to a wired LAN port on the Flytrap.
Ensure the default connection type for the wired interface is
DHCP.
c. On the Target laptop, open a browser and point it to the
Flytrap’s IP address (see section 8 Appendix for device specific
default addresses/usernames/passwords).
d. Set Flytrap Connection Type (or similar) to Static IP Address.
e. Set Flytrap IP address to an IP address on the same subnet as
the Squid Laptop (prevent an IP address conflict by first pinging
this address from the Squid Laptop).
f. Set Flytrap Default Gateway to the IP address of the Squid
Laptop.
g. Set Flytrap DNS to DNS address(es) used by Squid Laptop.
UNCLASSIFIED
15

- 1
- 2
…
- 13
- 14
- 15
- 16
- 17
…
- 79
- 80